For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
Schematic Reference: Audible Warnings Schematics
1 | Did you review the Audible Warning Description and Operation and perform the necessary inspections? | Go to Step 2 | Go to Symptoms - Instrument Panel, Gages and Console
2 | Verify that the chime is always on. Does the system operate normally? | Go to Testing for Intermittent Conditions and Poor Connections in Wiring Systems | Go to Step 3
3 | Remove the door jamb switch connector. Does the audible warning remain ON? | Go to Step 5 | Go to Step 4
4 | Replace the LH front door jamb switch. Refer to Front Side Door Jamb Switch Replacement in Lighting Systems. Did you complete the repair? | Go to Step 8 | --
5 |

1. Reconnect the LH front door jamb switch connector.
2. Disconnect the ignition key alarm switch.

Does the alarm stop sounding?

Go to Step 6

Go to Step 7

6 | Replace the ignition switch. Is the repair complete? | Go to Step 8 | --
7 | Replace the multifunction alarm module. Refer to Multifunction Alarm Module Replacement . Is the repair complete? | Go to Step 8 | --
8 | Operate the system in order to verify the repair. Did you correct the condition? | System OK | Go to Step 3