For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Wiper/Washer System Check? | -- | Go to Step 2 | Go to Wiper/Washer Rear System Check
2 |

1. Turn ignition switch to ON.
2. Disconnect the rear wiper/washer switch connector.

Does the rear motor continue to operate?

--

Go to Step 3

Go to Step 4

3 | Repair the short to voltage in the ORN wire between the rear wiper/washer switch and the rear wiper motor. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Wiper/Washer Rear System Check | --
4 |

1. Connect a J 39200 Digital Multimeter (DMM) across rear wiper/washer switch cavities 1-4.
2. Measure the resistance.

Is the resistance less than specified value?

∞

Go to Step 6

Go to Step 5

5 | Replace the rear wiper motor. Refer to Rear Window Wiper Motor Replacement . Is the repair complete? | -- | Go to Wiper/Washer Rear System Check | --
6 | Replace the rear wiper/washer switch. Windshield Wiper and Washer Switch Replacement . Is the repair complete? | -- | Go to Wiper/Washer Rear System Check | --