For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel steering column opening trim plate. Refer to Instrument Panel Trim Panel Replacement - Left Side in Instrument Panel, Gages and Console.
2. Slide the LOCK or the UNLOCK relay from the remote control door lock receiver bracket.
3. Remove the relay (1) from the relay connector (2).

### Installation Procedure

1. Install the relay (1) to the relay connector (2).
2. Slide the relay onto the remote control door lock receiver bracket.
3. Install the instrument panel steering column opening trim plate. Refer to Instrument Panel Trim Panel Replacement - Left Side in Instrument Panel, Gages and Console.