For 1990-2009 cars

1. Disconnect the brake pedal pushrod (1) from the brake pedal.
2. Inspect the brake pedal pushrod clevis (2) for cracks and/or excessive wear.
3. Reposition the pedal pushrod boot (3) toward the front of the vehicle in order to expose as much of the pedal pushrod as possible.
4. Inspect the brake pedal pushrod for straightness.
5. If the brake pedal pushrod clevis exhibits cracks and/or excessive wear, then replace the clevis.
6. If the brake pedal pushrod is not straight, then replace the brake booster order to replace the brake pedal pushrod.
7. Return the pedal pushrod boot to its original position on the pedal pushrod.
8. Connect the brake pedal pushrod to the brake pedal.