For 1990-2009 cars

#### Tools Required

• | J 41681 Clutch Spring Compressor

• | J 23327 Clutch Spring Compressor

1. Remove the brake apply cover bolts.
2. Remove the brake apply cover (1).
3. Remove the gasket.
4. Compress the reverse brake piston using J 41681 and J 23327 .
5. Remove the snap ring.
6. Remove the return springs (1).
7. Remove the retainer.
8. Cover the reverse brake piston with a clean cloth.
9. Slowly apply low pressure compressed air to the fluid passage B (2) while holding the fluid passage A (1) closed until the pistons are released from the case.
10. Remove the following loose components from the case.

• | The outer reverse brake piston (1)

• | The reaction sleeve (2)

• | The inner reverse brake piston (3)

11. Remove the piston O-ring seals.