For 1990-2009 cars

### Removal Procedure

Important: Before you remove the front wiper arm, note the wiper arm location for proper installation.

1. Remove one retaining nut from the front wiper arm (2).
2. Remove the front wiper arm (2) from the front wiper linkage (3).

### Installation Procedure

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

Install the front wiper arm (2) to the front wiper linkage (3). Secure the front wiper arm (2) with the retaining nut.

Tighten
Tighten the front wiper arm retaining nut to 20 N·m (15 lb ft).