For 1990-2009 cars

### Removal Procedure

1. Unzip the armrest trim and pull back to access the bolt.
2. Remove the bolt from the armrest.
3. Remove the armrest from the front bucket seat.

### Installation Procedure

1. Position the bolt into the mounting point of the armrest.
2. Position the armrest to the front bucker seat.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Tighten the armrest mounting bolt.

Tighten
Tighten the armrest mounting bolt to 4.5 N·m (40 lb in).

4. Zip up the armrest trim .
5. Inspect the armrest for proper movement.