For 1990-2009 cars

### Removal Procedure

1. Disconnect the reading lamp electrical connector if equipped.
2. Turn the inside rearview mirror arm 90 degrees counterclockwise in order to release the arm of the mirror from the mounting base.
3. Remove the inside rearview mirror from the vehicle.

### Installation Procedure

1. Install the inside rearview mirror to the mounting base by sliding the arm into the base. Secure the inside rearview mirror arm by turning 90 degrees clockwise.
2. Connect the reading lamp electrical connector if equipped.