For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
1 | Did you review the system Descriptions and perform the necessary inspections? | Go to Step 2 | Go to Symptoms - Suspension General Diagnosis
2 | Verify that the ride is too soft. Is the ride too soft? | Go to Step 3 | System OK
3 |

1. Inspect the vehicle trim height. Refer to Trim Height Inspection .
2. Replace components as necessary.

Did you replace any components?

Go to Step 6

Go to Go to Step 4

4 | Inspect the following components for wear or damage:

• | Front springs

• | Front struts

• | Rear springs

• | Rear shock absorbers

Refer to Suspension Strut and Shock Absorber Testing - On Vehicle .

Are any of the components worn or damaged?

Go to Step 5

Go to Step 2

5 | Replace all of the worn or damaged components. Refer to the following procedures:

• | Front Coil Springs Replacement in Front Suspension

• | Strut Assembly Replacement in Front Suspension

• | Coil Spring Replacement in Rear Suspension

• | Shock Absorber Replacement in Rear Suspension

Did you complete the repair?

Go to Step 6

--

6 | Drive the vehicle in order to verify the repair. Did you correct the condition? | System OK | Go to Step 2