For 1990-2009 cars

## Brake Pipe Replacement Front Without ABS

### Removal Procedure

1. Clean any dirt and foreign materials from the pipes and fittings.
2. Disconnect the pipe(s) (1) to be replaced at each fitting.
3. Remove the pipe(s) (1) from the guide brackets (3).
4. Remove the pipe(s) (1) from the vehicle.

### Installation Procedure

1. Install the brake pipe(s) (1) to each fitting.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Secure the pipes with guide brackets (3) and pipe fitting nuts (2).

Tighten
Tighten the brake pipe fitting nuts (2) to 16 N·m (12 lb ft).

3. Flush the brake system. Refer to Hydraulic Brake System Flushing in this section.

## Brake Pipe Replacement Rear Without ABS

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Clean any dirt and foreign materials from the pipes and fittings.
3. Remove the pipe guide clamps (2).
4. Disconnect the pipe(s) (1) to be replaced at each fitting.
5. Remove the pipe(s) from the vehicle.

### Installation Procedure

1. Install the brake pipe(s) (1) to the vehicle. Secure the pipe(s) at the respective guide clamps (2) and pipe fitting nuts.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the pipe guide clamps.

Tighten
Tighten the brake pipe fitting nuts to 16 N·m (12 lb ft).

3. Flush and bleed the brake system. Refer to Hydraulic Brake System Flushing in this section.

## Brake Pipe Replacement Front With ABS

### Removal Procedure

1. Clean any dirt and foreign materials from the pipes and fittings.
2. Disconnect the pipe(s) (1) to be replaced at each fitting.
3. Remove the pipe(s) (1) from the guide brackets (3).
4. Remove the pipe(s) (1) from the vehicle.

### Installation Procedure

1. Install the brake pipe(s) (1) to each fitting.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Secure the pipes with guide brackets (3) and pipe fitting nuts (2).

Tighten
Tighten the brake pipe fitting nuts (2) to 16 N·m (12 lb ft).

3. Flush the brake system. Refer to Hydraulic Brake System Flushing in this section.

## Brake Pipe Replacement Rear With ABS

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Clean any dirt and foreign materials from the pipes and fittings.
3. Remove the pipe guide clamps (2).
4. Disconnect the pipe(s) (1) to be replaced at each fitting.
5. Remove the pipe(s) from the vehicle.

### Installation Procedure

1. Install the brake pipe(s) (1) to the vehicle. Secure the pipe(s) at the respective guide clamps (2) and pipe fitting nuts.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the pipe guide clamps.

Tighten
Tighten the brake pipe fitting nuts to 16 N·m (12 lb ft).

3. Flush and bleed the brake system. Refer to Hydraulic Brake System Flushing in this section.