For 1990-2009 cars

### Removal Procedure

• | J 29792 Front Control Arm Bushing Service Set

• | J 35561 Front Control Arm Bushing Service Set

1. Remove the rear suspension upper control arm from the vehicle.

Refer to Upper Control Arm Replacement in this section.

2. Use the J 29792 and the J 35561 in order to mount the upper control arm (1) into a press.
3. Use a press in order to remove the bushing from the upper control arm.

### Installation Procedure

• | J 29792 Front Control Arm Bushing Service Set

• | J 35561 Front Control Arm Bushing Service Set

1. Use the J 29792 , the J 35561 and a press in order to install a new bushing (2) into the upper control arm (1).
2. Install the upper control arm to the vehicle. Refer to Upper Control Arm Replacement in this section.