For 1990-2009 cars

### Removal Procedure

1. Remove the 3 screws from the steering column lower trim cover (2).
2. Remove the steering column lower trim cover (2).
3. Remove the steering column upper trim cover (1).

### Installation Procedure

1. Install the steering column upper trim cover (1) to the steering column.
2. Install the steering column lower trim cover (2) to the steering column.
3. Secure the steering column lower trim cover with the 3 screws (2).