For 1990-2009 cars

### Removal Procedure

1. Push in the folding top latch buttons (2).
2. Pull the latch (1) back in order to unhook the latch (1) from the front top bow.
3. Remove the 2 folding top latch screws.
4. Remove the folding top latch from the vehicle.

### Installation Procedure

1. Install the folding top latch to the vehicle. Secure the folding top latch with the 2 screws.
2. Move the front top bow forward in order to hook the folding top latch.
3. Push the latch (1) down until the latch clicks into place.