For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Coolant Solution Protection Point | 36 °C | -33 °F
Cooling System Pressure Capacity | 90 kPa | 13 psi
Generator/Coolant Pump Drive Belt Deflection | 5-8 mm at 10 kg applied pressure | 0.20-0.32 in at 22 lbs applied pressure
Radiator Cap Pressure Capacity | 90 kPa | 13 psi
Thermostat Valve Lift (Minimum) | 8 mm at 95 °C | 0.31 in at 203 °F
Thermostat Valve Opening Temperature | 80-90 °C | 176-203 °F