For 1990-2009 cars

Caution: Refer to Brake Fluid Irritant Caution in the Preface section.

Caution: Refer to Brake Fluid Caution in the Preface section.

Notice: Refer to Filling the Master Cylinder Notice in the Preface section.

1. Install the reservoir to the master cylinder. Refer to Master Cylinder Reservoir Replacement .
2. Fill the master cylinder reservoir with brake fluid and keep full throughout the entire bleeding process.
3. Install adapters into each master cylinder outlet port.
4. Attach a piece of plastic tubing to each adapter and submerge the other ends in the reservoir. Ensure the tubes remain submerged in the fluid.
5. Using a wooden or plastic dowel, slowly push in the master cylinder piston and release. Repeat the process until there is no sign of air in the brake fluid.