For 1990-2009 cars

### Removal Procedure

1. Remove the front seat. Refer to Front Seat Replacement - Bucket .
2. Remove the front seat inner adjuster finish cover. Refer to Front Seat Adjuster Track Finish Cover Replacement .
3. Remove the front seat outer adjuster finish cover. Refer to Front Seat Adjuster Track Finish Cover Replacement .
4. Remove the front seat cushion. Refer to Front Seat Cushion Replacement
5. Lift the retaining springs (3, 4) and remove the seat adjuster handle (1) from the seat adjusters (2, 5).

### Installation Procedure

1. Install the seat adjuster handle (1) to the seat adjusters (2, 5). Ensure that the handle is locked into position by the retaining springs (3, 4).
2. Install the front seat cushion. Refer to Front Seat Cushion Replacement
3. Install the front seat outer adjuster finish cover. Refer to Front Seat Adjuster Track Finish Cover Replacement .
4. Install the front seat inner adjuster finish cover. Refer to Front Seat Adjuster Track Finish Cover Replacement .
5. Install the front seat. Refer to Front Seat Replacement - Bucket .