For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
DEFINITION: Low clutch pedal or pedal on the floor.
1 | Check the hydraulic fluid in the clutch master cylinder reservoir. Is the reservoir full? | Go to Step 3 | Go to Step 2
2 | Fill the reservoir with fluid. Does the clutch pedal still stay on the floor when disengaged? | Go to Step 3 | System OK
3 | Inspect the master cylinder. Does the master cylinder function properly? | Go to Step 5 | Go to Step 4
4 | Replace the master cylinder. Refer to Clutch Master Cylinder Replacement . Does the clutch pedal still stay on the floor when disengaged? | Go to Step 5 | System OK
5 | Check the hydraulic line for a hole or leaks. Is the line OK? | Go to Step 7 | Go to Step 6
6 | Replace the hydraulic line. Does the clutch pedal still stay on the floor when disengaged? | Go to Step 7 | System OK
7 | Check to see if the master cylinder pushrod has fallen off the clutch pedal. Has the master cylinder pushrod fallen off the clutch pedal? | Go to Step 8 | Go to Step 9
8 | Correctly install the master cylinder pushrod. Refer to Clutch Master Cylinder Replacement . Does the clutch pedal still stay on the floor when disengaged? | Go to Step 9 | System OK
9 | Inspect the clutch release bearing for binding. Is there binding on the clutch release bearing? | Go to Step 10 | System OK
10 | Lubricate and free-up the clutch release bearing or replace the clutch actuator. Refer to Clutch Actuator Cylinder Replacement . Does the clutch pedal still stay on the floor when disengaged? | -- | System OK