For 1990-2009 cars

Notice: If the power steering system has been serviced, an accurate fluid level reading cannot be obtained unless air is bled from the steering system. The air in the fluid may cause pump cavitation noise and may cause pump damage over a period of time.

Notice: When adding fluid or making a complete fluid change, always use the proper power steering fluid. Failure to use the proper fluid will cause hose and seal damage and fluid leaks.

The remote power steering fluid reservoir is at the left front corner of the engine compartment.

1. Remove the reservoir cap.
2. Check the fluid level on the cap fluid lever indicator (dipstick).
3. If the fluid does not reach the MAX mark on the indicator, add the power steering gear and pump fluid Dexron® -III Automatic Transmission Fluid GM P/N 12346143, or the equivalent.