For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
1 | Did you review the Exterior Lights Circuit Description and perform the necessary inspections? | Go to Step 2 | Go to Symptoms - Lighting Systems
2 | Verify that the Hazards are inoperative. Do the Hazards work normally? | Go to Testing for Intermittent Conditions and Poor Connections | Go to Step 3
3 |

1. Disconnect the Turn/Hazard Flasher connector.
2. Connect a test lamp between cavity 2 of the Turn/Hazard Flasher and ground.

Does the test lamp illuminate?

Go to Step 4

Go to Step 5

4 |

1. Push the Hazard Switch to the ON position.
2. Connect the fused jumper wire between cavity 2 and terminal 3 of the Turn/Hazard Flasher.

Do the hazard lamps illuminate?

Go to Step 6

Go to Step 7

5 | Repair the open condition in the BLK wire from the junction block to S207. Refer to Wiring Repairs in Wiring Systems. Did you complete the repair? | Go to Step 10 | --
6 | Replace the Turn/Hazard Flasher. Refer to Hazard and Turn Signal Flasher Replacement . Did you complete the repair? | Go to Step 10 | --
7 |

1. Reconnect the Turn/Hazard Flasher connector.
2. Disconnect the Hazard Switch connector.
3. Connect a fused jumper wire between cavity 1 and cavity 3 of the Hazard Switch assembly .

Does the left front turn lamp flash?

Go to Step 8

Go to Step 9

8 | Replace the Hazard Switch assembly. Did you complete the repair? | Go to Step 10 | --
9 | Repair the open in the GRN wire from the Turn/Hazard Flasher and the Hazard Switch. Refer to Wiring Repairs in Wiring Systems. Did you complete the repair? | Go to Step 10 | --
10 | Operate the system in order to verify the repair. Did you correct the condition? | System OK | Go to Step 3