For 1990-2009 cars

• | Dirt will cause premature wear of the rebuilt engine. Clean all the components.

• | Use the proper tools to measure the components when checking for excessive wear. Components not within the manufacturer's specification must be repaired or replaced.

• | When the components are reinstalled into an engine, return the components to their original location, position, and direction.

• | During assembly, lubricate all the moving parts with clean engine oil (unless otherwise specified). This will provide initial lubrication when the engine is first started.