For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Automatic Locking Hub Bolts | 33 N·m | 24 lb ft
Ball Stud Castle Nut | 58 N·m | 43 lb ft
Ball Stud Nuts and Bolts | 85 N·m | 63 lb ft
Brake Caliper Carrier Bolts | 88 N·m | 65 lb ft
Control Arm-to-Chassis Front Through Bolts and Nuts | 85 N·m | 62 lb ft
Control Arm-to-Chassis Rear Through Bolts and Nuts | 115 N·m | 84 lb ft
Cruise Control Bracket | 10 N·m | 89 lb in
Dust Shield Bolts | 15 N·m | 11 lb ft
Engine Skid Plate Bolts | 54 N·m | 40 lb ft
Engine Wiring Harness Bracket | 10 N·m | 89 lb in
Hub Bolts to the J 42119-1 and the J 42119-2 | 2.5 N·m | 12.12 lb in
Manual Locking Hub Bolts | 33 N·m | 24 lb ft
Spindle Nut | 210 N·m | 155 lb ft
Stabilizer Link-to-Control Arm Nut | 28 N·m | 21 lb ft
Stabilizer Shaft Mounting Bracket Bolts | 25 N·m | 18 lb ft
Stabilizer Shaft Mounting Bracket Nuts | 85 N·m | 62 lb ft
Stabilizer Shaft-to-Link Nuts | 50 N·m | 37 lb ft
Strut-to-Knuckle Bolts and Nuts | 90 N·m | 66 lb ft
Strut Upper Support Nuts | 25 N·m | 18 lb ft
Tie Rod End Castle Nut | 40 N·m | 30 lb ft
Wheel Speed Sensor Harness Bolt | 10 N·m | 89 lb in
Wheel Speed Sensor Retaining Bolt | 10 N·m | 89 lb in