For 1990-2009 cars

1. Install the detent valve spring (108) and spring seat (109) over the detent cable.
2. Connect the detent cable to the detent valve (110).
3. Install a new detent valve sleeve seal (113).
4. Install the detent valve (110) into the sleeve (111). Lubricate the valve and sleeve with DEXRON®III transmission fluid.
5. Install the detent sleeve assembly (111) into the transmission case. The slots face the oil pan mating surface.
6. Install the detent valve retaining pin (112).