For 1990-2009 cars

• | Inspect the disc brake pads at least twice a year, or whenever the tire and wheel assemblies are not on the vehicle.

• | The disc brake pads have wear indicators. When the pad lining wear reaches the minimum thickness, the wear indicator contacts the brake rotor (2). The wear indicator will produce a high-pitched warning noise during wheel rotation.

• | Inspect the thickness of the pad linings in order to verify that they have not worn unevenly. The pad lining wear should be approximately even per axle set. Compare the pad lining thickness to the following specification:

Specification
The minimum brake pad lining thickness is 2 mm (0.080 in)

• | Replace the disc brake pads when the pad lining thickness is less than the minimum specification.

• | Inspect both edges of the pad linings. The highest rate of wear normally occurs at the trailing edge of the disc brake pads.

• | Remove the calipers and inspect the lining surfaces of the inner and outer pads in order to verify that they are level. Place the pad lining surfaces together and measure the gap between the surfaces. If more than 0.13 mm (0.005 in) gap exists midway between the attaching lugs, replace the disc brake pads.

• | Verify that the brake pad insulators are in place and not damaged or excessively corroded. Replace any missing or damaged insulators in order to preserve proper disc brake performance.

• | Replace the disc brake pads if any linings have de-laminated from the mounting plates.

• | Inspect the disc brake pad lining surfaces for cracks or fractures which can cause noise or otherwise impair disc brake performance.

• | If replacement is necessary, always replace disc brake pads in axle sets. Refer to Brake Pads Replacement .