For 1990-2009 cars

1. Install the following primary regulator valve components:

• | The valve (4)

• | The spring (3)

• | The plunger (2)

• | The sleeve (1)

• | The sleeve retainer

2. Install the following TCC lock-up control valve components:

• | The spring

• | The sleeve

• | The locating pin

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the following shift solenoid components:

• | The intermediate coast modulator valves (5)

• | The intercoast modulator valve spring (2)

• | The low coast modulator valve spring (6)

• | The gasket

• | The solenoid (3)

• | The bolts

Tighten
Tighten the bolts to 10 N·m (89 lb in).

4. Install a new O-ring (2) to the TCC solenoid.
5. Lubricate the new O-ring with A/T fluid.
6. Install the TCC solenoid (1).
7. Install the TCC solenoid bolt.

Tighten
Tighten the bolt to 5 N·m (44 lb in).

8. Install the following pressure relief valve components:

• | The ball

• | The spring

• | The retainer (1)

• | The bolt

Tighten
Tighten the bolt to 5 N·m (44 lb in).

9. Install the following TCC lock-up control valve plate components:

• | The gasket

• | The plate (2)

• | The bolts

Tighten
Tighten the bolts to 5 N·m (44 lb in).

10. Install the following lower valve body plate components:

• | The gasket

• | The plate (1)

• | The bolts

Tighten
Tighten the bolts to 5 N·m (44 lb in).

11. Install the following components to the valve body:

• | The ball valve spring

• | The valve body ball (2)

• | The valve dampening spring

• | The check ball (6)

• | The bypass valve spring

• | The bypass valve (3)