For 1990-2009 cars

### Removal Procedure

1. Lower the rear side door window completely.
2. Remove the screw (2) which secures the rear side door window outer sealing strip (1).
3. Use a flat-bladed tool wrapped in tape in order to gently pry the outer sealing strip (1) from the rear side door (3).

### Installation Procedure

1. Install the rear side door window outer sealing strip (1) to the rear side door (3) by pressing into place. Secure the strip with the screw (2).
2. Raise the rear side door window.