For 1990-2009 cars

## Folding Top Weatherstrip Replacement Front

### Removal Procedure

1. Remove the folding top #1 bow. Refer to Folding Top Roof Bow Replacement .
2. Fold the front folding top material (1) back in order to gain access to the folding top front weatherstrip (4).
3. Remove the folding top front weatherstrip (4) from the roof opening pinch flange.

### Installation Procedure

1. Install the folding top front weatherstrip (4) to the roof opening pinch flange.
2. Install the folding top #1 bow. Refer to Folding Top Roof Bow Replacement .