For 1990-2009 cars

### Removal Procedure

1. Remove the brake pads and the hardware. Refer to Brake Pads Replacement .
2. Remove the 2 mounting bolts and the caliper bracket (2) from the vehicle.
3. Remove the 2 caliper pins and the 2 boots from the caliper bracket.

### Installation Procedure

Important: Verify the boots fit into the grooves securely.

1. Install the 2 boots to the caliper bracket.
2. Apply disc brake caliper lubricant to the slide pins.
3. Install the slide pins to the caliper bracket.
4. Install the caliper bracket (2) to the vehicle.

Notice: Refer to Fastener Notice in the Preface section.

5. Install the 2 mounting bolts.

Tighten
Tighten the bolts to 85 N·m (61.5 lb ft).

6. Install the brake pads and the hardware. Refer to Brake Pads Replacement .