For 1990-2009 cars

1. Fill the reservoir with new fluid. Use Hydraulic Clutch Fluid (GM P/N 12345347) (Canadian P/N 10953517) or equivalent.
2. Depress the clutch pedal (hold the pedal down).
3. Open the bleed screw on the clutch actuator cylinder in order to expel the air.

Important: Ensure no air is drawn into the clutch system.

4. Close the bleed screw then release the clutch pedal.
5. Repeat steps 2, 3, and 4 until all the air is out of the clutch system.
6. Check and refill the reservoir as needed while bleeding.
7. After bleeding, pump the clutch pedal several times. If the clutch engagement is not satisfactory, repeat the bleeding procedure.