For 1990-2009 cars

### Removal Procedure

1. Remove the 2 screws (2) which secure the front side marker lamp (1).
2. Pull the front side marker lamp (3) from the front bumper fascia.
3. Twist the side marker bulb socket (1) counterclockwise and remove the socket from the front side marker lamp (3).
4. Remove the front side marker lamp (3) from the vehicle.
5. Remove the bulb (2) from the socket (1), if necessary.

### Installation Procedure

1. Install the bulb (2) to the socket (1), if removed.
2. Install the front side marker lamp bulb socket (1) to the front side marker lamp (3) and twist clockwise in order to secure.
3. Install the front side marker lamp (1) to the front bumper fascia. Secure the lamp with the 2 screws (2).