For 1990-2009 cars

## Front Fender Lower Molding Replacement LT Models

### Removal Procedure

1. Use a taped flat bladed tool or a taped trim tool in order to release the 3 plastic retainers that retain the front fender lower molding (1). Release the front fender lower molding beginning at the bottom of the molding.
2. Remove the front fender lower molding (1) from the vehicle.
3. Remove the 3 plastic retainers from the front fender and/or the fender lower molding (1).

### Installation Procedure

1. Install the 3 plastic retainers to the front fender lower molding (1). Replace any retainers that were damaged in the removal process.
2. Install the front fender lower molding (1) to the front fender. Make certain that the plastic retainers are completely engaged.