For 1990-2009 cars

### Removal Procedure

#### Tools Required

J 24319-B Universal Steering Linkage Remover

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the 4 bolts from the engine skid plate.
3. Remove the engine skid plate.
4. Remove the following fasteners securing the tie rod to the center link:

4.1. | The cotter pin

4.2. | The castle nut

5. Use the J 24319-B in order to remove the tie rod from the center link.

Important: For ease of adjustment after installation, mark the position of the tie rod locknut on the tie rod thread.

6. Loosen the tie rod locknut (2) at the connector sleeve (3).
7. Remove the tie rod (1) from the connector sleeve (3).
8. Remove the locknut (2) from the tie rod (1).
9. Inspect the tie rod dust seal for a perforation or excessive wear.

Replace the seal if you find a perforation or excessive wear.

### Installation Procedure

1. Install the locknut (2) to the tie rod (1).

Do not tighten the locknut. Align the marks denoting the position of the tie rod locknut (2) with the tie rod thread.

2. Thread the tie rod into the connector sleeve (3).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the tie rod to the center link with the castle nut .

Tighten

• | Tighten the tie rod castle nut to 45 N·m (33 lb ft).

• | Tighten the tie rod locknut to 65 N·m (48 lb ft).

4. Install the cotter pin to the tie rod shaft.

Bend the end of the pin following the installation.

5. Inspect for the proper toe adjustment. Refer to Wheel Alignment Measurement in Wheel Alignment.
6. Install the engine skid plate, if equipped.

Secure the engine skid plate with the 4 bolts.

Tighten
Tighten the engine skid plate bolts to 27 N·m (20 lb ft).

7. Lower the vehicle.