For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Battery Cable-to-Battery Terminal Retainers | 15 N·m | 11 lb ft
Battery Hold Down Bracket Nuts | 8 N·m | 71 lb in
Body Ground Bolt | 8 N·m | 71 lb in
Camshaft Position (CMP) Sensor Retaining Screws | 15 N·m | 11 lb ft
Commutator End Cover Bolts | 8 N·m | 71 lb in
Field Coil Lead Wire Retaining Nut | 10 N·m | 89 lb in
Generator B Terminal Nut | 10 N·m | 89 lb in
Generator Housing Bolts | 17 N·m | 10 lb ft
Generator Mounting Bolts | 23 N·m | 17 lb ft
Generator Pulley Nut | 118 N·m | 86 lb ft
Ignition Coil Bolts | 10 N·m | 89 lb in
Solenoid Mounting Screws | 7 N·m | 62 lb in
Spark Plugs | 25 N·m | 19 lb ft
Starter Motor Mounting Bolts | 30 N·m | 22 lb ft
Starter Solenoid Nut | 8 N·m | 71 lb in