For 1990-2009 cars

## High Mount Stop Lamp Bulb Replacement 2-Door

### Removal Procedure

1. Remove the 2 screws and the high-mounted stop lamp from the housing.
2. Remove the bulb socket from the lens.
3. Remove the bulb from the bulb socket.

### Installation Procedure

1. Install the bulb to the bulb socket. Secure the bulb socket to the lens.
2. Install the lens to the housing. Secure the lens with the 2 screws.

## High Mount Stop Lamp Bulb Replacement 4-Door

### Removal Procedure

1. Open the rear door.
2. Remove the 2 clips which secure the high-mounted stoplamp housing.
3. Remove the high-mounted stoplamp housing from the lamp.
4. Remove the bulb socket from the lens.
5. Remove the bulb from the bulb socket.

### Installation Procedure

1. Install the bulb to the bulb socket. Secure the bulb socket to the lens.
2. Install the housing to the lamp. Secure the housing with the 2 clips.
3. Close the rear door.