For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Air Cleaner (ACL) Mounting Bolts | 10 N·m | 89 lb in
Air Conditioner (A/C) Compressor Mounting Bolts | 23 N·m | 17 lb ft
Air Conditioner (A/C) Compressor Bracket Mounting Bolts | 55 N·m | 40 lb ft
Camshaft Bearing Cap Bolts | 11 N·m | 97 lb in
Camshaft Position Sensor Bolt | 15 N·m | 11 lb ft
Camshaft Timing Sprocket Bolts | 80 N·m | 58 lb ft
Connecting Rod Bearing Cap Nuts | 45 N·m | 33 lb ft
Coolant Bypass Pipe to Cylinder Head Bolt | 15 N·m | 11 lb ft
Crankshaft Position Sensor Bolt | 6 N·m | 53 lb in
Crankshaft Pulley Bolt | 150 N·m | 109 lb ft
Cylinder Head Cover Bolts | 11 N·m | 97 lb in
Cylinder Head Bolts

- First Pass

53 N·m

39 lb ft

- Second Pass

84 N·m

61 lb ft

- Third Pass

Loosen to 0

- Fourth Pass

53 N·m

39 lb ft

- Fifth Pass

84 N·m

61 lb ft

- Sixth Pass (Final Torque)

105 N·m

76 lb ft

Cylinder Head M 6 Bolt | 11 N·m | 97 lb in
Drive Belt Idler Pulley Nut | 45 N·m | 33 lb ft
Drive Belt Tensioner Bolts

- Cooling Fan Drive Belt Tensioner Bolts

45 N·m

33 lb ft

- Accessory Drive Belt Tensioner Bolts

25 N·m

19 lb ft

Engine Cooling Fan Nuts | 11 N·m | 97 lb in
Engine Ground Wire Bolts | 15 N·m | 11 lb ft
Engine Mount Bracket Bolts (Engine Side) | 50 N·m | 37 lb ft
Engine Mount Bracket Bolts (Body Side) | 85 N·m | 62 lb ft
Engine Mount Nuts | 50 N·m | 37 lb ft
Engine Oil Drain Plug | 35 N·m | 26 lb ft
Engine Oil Pan Nuts and Bolts | 11 N·m | 97 lb in
Exhaust Manifold Flange Bolts | 50 N·m | 37 lb ft
Exhaust Manifold Heat Shield Bolts | 15 N·m | 11 lb ft
Exhaust Manifold-to-Cylinder Head Nuts | 50 N·m | 37 lb ft
Exhaust Manifold-to-Bracket Bolts | 50 N·m | 37 lb ft
Exhaust Pipe PUP Catalytic Converter Clamp Bolt | 50 N·m | 37 lb ft
Fuel Rail to Cylinder Head Bolts | 23 N·m | 17 lb ft
Fuel Rail Banjo Fitting | 30 N·m | 22 lb ft
Flywheel Retaining Bolts

- Automatic Transmission

70 N·m

51 lb ft

- Manual Transmission

70 N·m

51 lb ft

Generator Mounting Bolts and Nuts | 23 N·m | 17 lb ft
Heated Oxygen (HO2S1 and HO2S2) Sensor | 45 N·m | 33 lb ft
Ignition Coil Bolts | 10 N·m | 89 lb in
Intake Manifold Bolts and Nuts | 25 N·m | 19 lb ft
Intake Manifold Front Support Bracket Bolts | 45 N·m | 33 lb ft
Intake Manifold Top Support Bracket Bolts | 15 N·m | 11 lb ft
Lower Crankcase Bolts

- First Pass

19 N·m

14 lb ft

- Second Pass (Final Torque)

27 N·m

20 lb ft

Main Bearing Cap Bolts:

- First Pass

42 N·m

31 lb ft

- Second Pass (Final Torque)

60 N·m

44 lb ft

Negative Battery Cable | 15 N·m | 11 lb ft
Oil Filter Adapter | 23 N·m | 17 lb ft
Oil Pressure Switch | 14 N·m | 11 lb ft
Oil Pump Sprocket Cover Bolts | 11 N·m | 97 lb in
Oil Pump Bolts | 27 N·m | 20 lb ft
Oil Pump Case Bolts | 12 N·m | 106 lb in
Oil Pump Strainer Bolts | 11 N·m | 97 lb in
Oil Pump Relief Valve Retainer | 29 N·m | 21 lb ft
Power Steering Pump Bolts | 25 N·m | 19 lb ft
Spark Plugs | 25 N·m | 18 lb ft
Starter Bolts | 30 N·m | 22 lb ft
Strut Tower Brace | 50 N·m | 37 lb ft
Throttle Body Bolts and Nuts | 25 N·m | 19 lb ft
Timing Chain Cover Nut and Bolts | 11 N·m | 97 lb in
Timing Chain Tensioner Bolts (Camshaft) | 11 N·m | 97 lb in
Timing Chain Tensioner Bolts (Crankshaft) | 11 N·m | 97 lb in
Timing Chain Tensioner Nut (Camshaft) | 45 N·m | 33 lb ft
Timing Chain Tensioner Guide Bolts (Crankshaft) | 9 N·m | 62 lb in
Timing Chain Tensioner Shoe Nut (Crankshaft) | 25 N·m | 19 lb ft
Torque Converter Bolts | 65 N·m | 47 lb ft
Transmission Bracket Bolts | 50 N·m | 37 lb ft
Transmission to Engine Mounting Bolts | 85 N·m | 62 lb ft
Water Pump Bolts | 27 N·m | 20 lb ft