For 1990-2009 cars

### Removal Procedure

1. Remove the 4 plastic retainers (1) from the top of the radiator grille (2).
2. Gently pull the radiator grille (2) from the vehicle by releasing the plastic retainers.

### Installation Procedure

1. Install the radiator grille (2) to the vehicle. Ensure that the plastic retainers are fully engaged.
2. Install the 4 plastic retainers (1) along the top of the radiator grille (2).