For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
1 | Did you review the Interior Lights Circuit Description and perform the necessary inspections? | Go to Step 2 | Symptoms - Lighting Systems
2 | Verify that the Instrument Panel Lamps are always on. Do the Instrument Panel operate normally? | Go to Testing for Intermittent Conditions and Poor Connections | Go to Step 3
3 | Disconnect the IP Cluster connector. Test for an open condition between connector C2, cavity 2 and S253. Does an open condition exist? | Go to Step 4 | Go to Step 5
4 | Repair the open in the RED/YEL wire from cavity 2 to S253. Refer to Wiring Repairs in Wiring Systems. Did you complete the repair? | Go to Step 9 | --
5 | Test for an open condition between connector C3, cavity 6 and S254. Does an open condition exist? | Go to Step 6 | Go to Step 7
6 | Repair the open condition between connector C3, cavity 6 and S254. Refer to Wiring Repairs in Wiring Systems. Did you complete the repair? | Go to Step 9 | --
7 | Inspect the Instrument Panel printed circuit for any damage or loose connections. Does any damage to the printed circuit exist? | Go to Step 8 | Go to Testing for Intermittent Conditions and Poor Connections
8 | Repair the Instrument Cluster printed circuit. Refer to Printed Instrument Cluster Circuit Replacement in Instrument Panel, Gages and Console. Did you complete the repair? | Go to Step 9 | --
9 | Operate the system in order to verify the repair. Did you correct the condition? | System OK | Go to Step 3