For 1990-2009 cars

## Quarter Lower Rear Trim Panel Replacement 2 Door

### Removal Procedure

1. Remove the screw from the front seat belt trim bezel (3).
2. Pull the rear quarter interior trim panel (1) from the vehicle, disengaging the plastic retainers.
3. Loosen the rear door opening weatherstrip.
4. Remove the 4 screws from the rear door sill plate (2).
5. Remove the rear door sill plate (2).
6. Remove the plastic retainers which secure the front of the rear floor carpet.
7. Pull the rear floor carpet away.
8. Remove the rear quarter wheelhousing trim panel from the vehicle.

### Installation Procedure

1. Install the rear quarter wheelhousing trim panel to the vehicle.
2. Place the rear floor carpet into position. Secure the carpet with the plastic retainer at the front of the rear floor carpet.
3. Install the rear door sill plate (2) to the vehicle. Secure the plate with the 4 screws.
4. Install the rear seat belt retractor trim panel to the vehicle. Secure the panel with the 2 plastic retainers.
5. Press the rear door opening weatherstrip into place.
6. Install the rear quarter interior trim panel (1) to the vehicle by pressing the panel into place. Ensure that the plastic retainers are fully engaged.
7. Install the front seat belt trim bezel (3) to the vehicle. Secure the bezel with the screw.

## Quarter Lower Rear Trim Panel Replacement 4 Door

### Removal Procedure

1. Remove the rear seat belt retractor trim panel (7). Refer to Rear Quarter Trim Panel Replacement .
2. Remove the rear quarter window interior trim (13). Refer to Rear Quarter Upper Trim Panel Replacement .
3. Remove the following from the vehicle:

3.1. | 1 push clip

3.2. | 2 screws

3.3. | The rear side door upper trim panel (9)

4. Remove the 2 screws which secure the rear side door sill plate.
5. Remove the rear side door sill plate.
6. Remove the 2 screws which secure the rear side door lower trim panel (8).
7. Remove the rear side door lower trim panel.
8. Remove the wheelhousing interior trim panel (6) from the vehicle.

### Installation Procedure

1. Install the wheelhousing interior trim panel (6) to the vehicle.
2. Install the rear side door lower trim panel to the vehicle. Secure the panel with the 2 screws and the push clip.
3. Install the rear side door upper trim panel to the vehicle. Secure the panel with the 2 screws.
4. Install the rear side door sill plate to the vehicle. Secure the panel with the 2 screws.
5. Install the rear quarter window interior trim. Refer to Rear Quarter Upper Trim Panel Replacement .
6. Install the rear seat belt retractor trim panel (7). Refer to Rear Quarter Trim Panel Replacement .