For 1990-2009 cars

### Removal Procedure

1. Remove the knee bolster. Refer to Knee Bolster Replacement .
2. Push on the bottom of the illumination controller by pushing up with a pick from behind the instrument panel.
3. Slide the illumination controller (2) out from the instrument panel.
4. Disconnect the electrical connector from the illumination controller (2).
5. Remove the illumination controller from the vehicle.

### Installation Procedure

1. Connect the electrical connector to the illumination controller (2).
2. Install the illumination controller (2) to the instrument panel.
3. Install the knee bolster. Refer to Knee Bolster Replacement .