For 1990-2009 cars

### Removal Procedure

1. Open the instrument panel compartment by pushing in on both sides to release the IP compartment door stops.
2. Remove the following components from the instrument panel:

2.1. | The screw (1)

2.2. | The instrument panel compartment (2)

### Installation Procedure

1. Install the instrument panel compartment (2) to the instrument panel. Secure the compartment with the screw (1).
2. Close the instrument panel compartment by pushing in on both sides.