For 1990-2009 cars

## Generator Bracket Replacement 1.6L

### Removal Procedure

1. Remove the generator from the vehicle. Refer to Generator Replacement .
2. Remove the bolt from the oil level indicator tube bracket.
3. Remove the 3 bolts (1) and the upper generator bracket (2) from the vehicle.
4. Remove the 1 nut and 1 bolt and the lower generator bracket from the vehicle.

### Installation Procedure

1. Install the upper generator bracket (2) to the vehicle. Secure with the 3 bolts (1).
2. Install oil level indicator tube bracket bolt.
3. Install the lower generator bracket to the vehicle. Secure with the 1 nut and 1 bolt.
4. Install the generator to the vehicle. Refer to Generator Replacement .

## Generator Bracket Replacement 2.0L

### Removal Procedure

1. Remove the generator from the vehicle. Refer to Generator Replacement .
2. Remove the 2 bolts and the upper generator bracket (1) from the vehicle.
3. Remove the 2 bolts and the lower generator bracket (2) from the vehicle.

### Installation Procedure

1. Install the upper generator bracket (1) to the vehicle. Secure with the 2 bolts.
2. Install the lower generator bracket (2) to the vehicle. Secure with the 2 bolts.
3. Install the generator to the vehicle. Refer to Generator Replacement .