For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Headlight System Check? | -- | Go to Step 2 | Go to Headlight System Check
2 | Are the high beams operational? | -- | Go to Step 3 | Go to Headlamps Inoperative - High Beams
3 |

1. Using a J 36169-A fused jumper wire, backprobe cavity 20 of the combination switch to ground.
2. Pull the combination switch to the PASS position.

Do the high beams operate?

--

Go to Step 5

Go to Step 4

4 | Replace the combination switch. Is the replacement complete? | -- | Go to Headlight System Check | --
5 | Repair the open BLK wire between cavity 20 of the combination switch and S214. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Headlight System Check | --