For 1990-2009 cars

### Removal Procedure

#### Tools Required

J 24319-B Universal Steering Linkage Remover

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the tire and wheel assembly from the vehicle. Refer to Wheel Removal in Tires and Wheels.
3. Remove the cotter pin and the castle nut from the tie rod end.

Important: For ease of adjustment after installation, mark the position of the tie rod end locknut on the tie rod thread.

4. Use the J 24319-B in order to separate the tie rod end (4) from the steering knuckle (5).
5. Loosen the tie rod end locknut (3).
6. Remove the tie rod end (4) from the tie rod connector sleeve.
7. Inspect the tie rod end dust seal for a perforation or excessive wear.

Replace the seal if you find a perforation or excessive wear.

### Installation Procedure

1. Install the tie rod end (5) and the locknut (4) to the tie rod connector sleeve (3).
2. Align the marks denoting the position of the tie rod end locknut with the tie rod thread.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the tie rod end to the steering knuckle. Secure the tie rod with the castle nut (7).

Tighten
Tighten the tie rod end castle nut to 45 N·m (33 lb ft).

4. Install the cotter pin (6) to the tie rod end.

Bend the end of the pin following the installation.

Tighten
Tighten the tie rod end locknut (4) to 65 N·m (48 lb ft).

5. Inspect for proper toe adjustment. Refer to Wheel Alignment Measurement in Tires and Wheels.
6. Install the tire and wheel assembly to the vehicle. Refer to Wheel Installation in Tires and Wheels.
7. Lower the vehicle.