For 1990-2009 cars

### Removal Procedure

1. Disconnect the stop lamp switch connector.
2. Remove the stop lamp switch nut (1) and the stop lamp switch (2).

### Installation Procedure

Important: DO NOT tighten the stop lamp switch nut before adjusting the stop lamp switch.

1. Install the stop lamp switch (2) to the bracket. Secure with the nut (1).
2. Connect the stop lamp switch connector.
3. Adjust the stop lamp switch. Refer to Stop Lamp Switch Adjustment .