For 1990-2009 cars

### Removal Procedure

1. Pull the quarter window reveal molding (3) away from the quarter window (2).
2. Remove the quarter window reveal molding (3) from the vehicle.

### Installation Procedure

Important: Trim the reveal molding (3), as needed, in order to fit the molding in the cavity between the quarter window (2) and the body.

1. Apply a bead of urethane adhesive from the urethane adhesive kit GM P/N 12346284 into the cavity between the quarter window (2) and the quarter window pillar.
2. Install the quarter window reveal molding (3) to the vehicle.
3. Starting from the center of the quarter window reveal molding (3), press the quarter window reveal molding into place.