For 1990-2009 cars

### Removal Procedure

1. Raise and suitably support the hood.
2. Remove the 2 bolts (2) and the hood primary latch (1) from the front upper panel.
3. Remove the hood primary latch release cable from the hood primary latch (1).
4. Unclip the hood primary latch release cable from the hold down clips.
5. Disconnect the hood primary latch release cable grommet from the body
6. Remove the hood primary latch release handle. Refer to Hood Primary Latch Release Cable Handle Replacement in Body Front End.
7. Attach a piece of mechanic's wire (1) to the hood primary latch release cable (2) in order to aid in the removal and the installation of the release cable.
8. Pull the hood primary latch release cable through the body.
9. Remove the hood primary latch release cable from the vehicle by pulling the cable from outside the engine compartment.

Important: The mechanic's wire should remain strung through the body in order to ease the installation of the hood latch release cable (2).

10. Remove the mechanic's wire (1) from the release cable (2).

### Installation Procedure

1. Attach the mechanic's wire (1) to the hood primary latch release cable (2).
2. Guide the hood primary latch release cable through the body with the mechanic's wire.
3. Remove the mechanic's wire (1) from the hood primary latch release cable (2).
4. Install the hood primary latch release cable grommet to the body, making sure the grommet is seated.
5. Install the hood primary latch release handle. Refer to Hood Primary Latch Release Cable Handle Replacement in Body Front End.
6. Install the hood primary latch release cable to the hold down clips.
7. Install the hood primary latch release cable to the hood primary latch (1).
8. Install the hood primary latch (1) to the front upper panel. Secure the latch with the 2 retaining bolts. Do not fully tighten the bolts.
9. Adjust the hood primary latch (1) in order to ensure that the striker shaft lines up with the center groove of the hood primary latch (1).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

10. Adjust the hood primary latch (1) in order to ensure that the hood is flush with the front fenders. Refer to Body Front End Adjustment Specifications .

Tighten
Tighten the hood latch retaining bolts to 10 N·m (89 lb in)

11. Lower the hood.