For 1990-2009 cars

### Removal Procedure

1. Remove the radio from the instrument panel. Refer to Radio Replacement in Entertainment.
2. Remove the screw which secures the IP ashtray lamp housing (1) to the instrument panel.
3. Disconnect the IP ashtray lamp electrical connector.
4. Remove the IP ashtray lamp housing (1) from the vehicle.
5. Remove the ashtray lamp bulb from the housing (1), if necessary.

### Installation Procedure

1. Install the IP ashtray lamp bulb to the IP ashtray lamp housing (1), if removed.
2. Connect the IP ashtray lamp electrical connector.
3. Install the IP ashtray lamp housing (1) to the instrument panel. Secure the housing with the screw.
4. Install the radio to the instrument panel. Refer to Radio Replacement in Entertainment.