For 1990-2009 cars

### Removal Procedure

1. Remove the front seat head restraint and the guides. Refer to Front Seat Head Restraint Replacement .
2. Release the J-retainer (2) on the bottom of the seat back cushion which secures the seat back cushion cover (1).
3. Roll the seat back cushion cover (1) up and off the seat back cushion (2).

### Installation Procedure

1. Roll the seat back cushion cover (1) onto the seat back cushion (2).
2. Secure the J-retainer (2) on the bottom of the seat back cushion which secures the seat back cushion cover (1).
3. Install the front seat head restraint and the guides. Refer to Front Seat Head Restraint Replacement .