For 1990-2009 cars

### Removal Procedure

1. Remove the grille. Refer to Grille Replacement in Exterior Trim.
2. Remove the 7 bolts (3) along the top of the front bumper fascia (4).
3. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General information.
4. Remove the 2 screws (5) and the 2 push pins (6) from the bottom of the front bumper fascia (4).
5. Remove 1 fascia screw at each wheelhousing (1).
6. Remove the fascia (4) from the vehicle.

### Installation Procedure

1. Install the front bumper fascia (4) to the vehicle. Secure the fascia (4) with the 2 screws (5) and the 2 push pins (6) along the bottom of the fascia.
2. Install 1 screw at each wheelhousing (1).
3. Lower the vehicle.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

4. Install the 7 bolts (3) along the top of the front bumper fascia.

Tighten
Tighten the front bumper fascia bolts to 15 N·m (11 lb ft).

5. Install the grille. Refer to Grille Replacement in Exterior Trim.