For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Brake Pedal Distance to Bulkhead | 80 mm with 294 N of force | 3.15 in with 66 lbs of force
Push Rod Clevis Length | 126.1-127.1 mm | 4.96-5 in
Stoplamp Switch-to-Brake Pedal Clearance | 1.5-2.0 mm | 0.06-0.08 in
Booster Piston Rod and Master Cyinder Piston Clearance:

- 2-Door Models Without ABS

0.25-0.5 mm

0.01-0.02 in

- All Other Models

0.14-0.35 mm

0.006-0.014 in

Low Hydraulic Brake Fluid Pressure Specifications (LSPV equipped)

- Front Brake Circuit Hydraulic Pressure

50 kg/cm²

711 psi

- Rear Brake Circuit Hydraulic Pressure

20 to 32 kg/cm²

285 to 455 psi

High Hydraulic Brake Fluid Pressure Specifications (LSPV equipped)

- Front Brake Circuit Hydraulic Pressure

100 kg/cm²

1422 psi

- Rear Brake Circuit Hydraulic Pressure

30 to 44 kg/cm²

427 to 625 psi