For 1990-2009 cars

### Tools Required

• | J 21474-01 Control Arm Bushing Set

• | J 35739 Control Arm Bushing Installer

• | Snap-on® A57Q Bushing Remover/Installer Set

### Removal Procedure

1. Remove the front suspension lower control arm. Refer to Lower Control Arm Replacement .
2. Spray penetrating lubricant on the bushings in order to loosen the bushings from the control arm.

Important: Do not transfer bushings from an old control arm to a new control arm.

3. Use a hydraulic press and adaptors or the following tools in order to remove the 2 bushings (7,10) from the control arm (11):

• | A vise

• | A hammer

• | The appropriate adaptors

### Installation Procedure

Important: New control arms do not include bushings. New bushings are available separately.

1. Apply Slick 50® One Lube, or an equivalent PTFE lubricant, or soap water, to the outside of a NEW front bushing (7) and the inside of the control arm housing.
2. Use a hydraulic press, or the following tools, or equivalent tools, in order to install the front bushing to the control arm:

• | Snap-on® A57-41 Adaptor

• | 2 Snap-on® A57Q Bearings

• | 2 Snap-on® A57Q Washers

• | J 21474-13 Adaptor

• | J 21474-18 Nut

• | J 21474-19 Screw

• | J 35739-3 Adaptor

3. Verify the flange of the bushing contacts the control arm.
4. Apply Slick 50® One Lube, or an equivalent PTFE lubricant, or soap water, to the outside of a NEW rear bushing (10) and the inside of the control arm housing.
5. Use a hydraulic press, or the following tools, or equivalent tools, in order to install the rear bushing to the control arm:

• | Snap-on® A57-3 Adaptor

• | Snap-on® A57-44 Adaptor

• | Snap-on® A57-47 Adaptor

• | 2 Snap-on® A57Q Bearings

• | Snap-on® A57Q Nut

• | Snap-on® A57CA Screw

• | 2 Snap-on® A57Q Washers

6. Verify the flange of the bushing contacts the control arm.
7. Install the control arm. Refer to Lower Control Arm Replacement .